Exported from SPITFIRE Bulletin Board System on 09-23-99 at 09:50:39.
DATE..... : 09-23-99 04:56:27
TO....... : Dave Nemeth
FROM..... : Al Robres
SUBJECT.. : Spitfire can Telnet

 Written by
 Al Robres
 baddog@linkline.com
 
 (Special SpitFire BBS 3.51 Edition)
 
 How to set up and use the new NetModem version 2.0
 
 Needed items:
 
     NetModem version 2.0 available at http://www.allensoftware.com
     Fossil Driver version 1.46 available at http://www.digsys.se
 
 Note: I could not get BNU or X00 to correctly initialize the modem
       in my BBS software. The author of NetModem has suggested using it.
       
 If you have any previous installations of NetModem (16) or version 1.4
 you must completely remove the program and use the utility called FIX.ZIP
 This utility will remove NetModem from your registry in Win9x. Also re-boot
 before starting any installation.
 
 Un-zip NETM_2A2.ZIP into a temp directory and run Setup.exe to begin the
 installation. After completion and re-booting your computer. You will need
 to go to "Settings" and your "Control Panel" to set up NetModem.
 
 There are basically 5 sections and you want to use a Comm port that your
 not using, as this will be a "Virtual Port"
 
 Section 1: Server
 
            [ ] Start as system service      [ ] Explicit bind to address
            [ ] Suppress splash screen       [ ] Allow unknown hosts *
            [x] Auto-minimize on startup     [ ] Display busy file *
            [x] Enable spinning globe        [ ] Display offline file *
            [x] Server logging               [x] Fake activity
               [x] Server activity              [10] minute intervals
               [x] User activity
               [x] Winsock activity          [x] Enable Auto-News
               [ ] Event activity *          [ ] Not ready! *
            
            [x] Retrieve local host info
            
               Advanced
               
                Available IRQ [9]                   Ring count [3]
                
                Internal cache size             TX/RX buffer size
                [ 2048KB ]                      [ 2048KB ]

 * meaning not used or disabled.
 
 The above is pretty much the default settings. Don't check "Start as system
 service" as there is a problem saving your configuration settings. What
 will happen is as you re-boot the computer. An error message will pop up
 warning you that NetModem is not properly configured and you must go to the
 Control Panel to configure it. Leave the box un-checked and you will be
 fine.
 
 Please note that the "Available IRQ" is adjustable and you need to select
 one that in not in use.
 
 ===========================================================================
 
 Section 2: Options
 
         [ Node 1 ]                     (x) Enabled  ( ) Disabled
 
         [ ] Caller ID *                [ ] Front-end mode *
         [ ] Call Block *               [ ] Display duplicate file *
         [ ] Call Forwarding *          [ ] Display blocked file *
         [ ] Allow dupe connections *   [ ] Display connect file *
         [ ] Activity log *             [ ] Display disconnect file *
         [ ] Play sound on connect      [ ] Display error file *
         [ ] Play sound on disconnect   [ ] Software compression
         [ ] Play sound on error        [ ] Limit bandwidth
         
 
 * meaning not used or disabled.
 
 ===========================================================================
 
 Section 3: Comports
 
         [ Node 1 ]
         
         COM1
         COM2
         COM3 <---Just make sure it's not in use. For our example
         COM4
         COM5
         COM6
         COM7
         COM8
         
         Emulation              Baudrate               Internet port
         [UART]                 [57600]                [23]
         
         UART Options                    Fossil Options
                                          [x] Always active
         Base/hex address                 [x] Locked baudrate
         [ 03E8 ]                         [ ] Manage time-slice
         
         Buffer size                     Buffer size
         [ 2048 KB ]                     [ 2048KB ]
 
 The Com Port you select will be the "Virtual Port" and should not be
 any ports your using like a mouse or modem. Make a note of the com
 and Base/hex address as these settings must be used in your BBS software
 settings.
 
 ===========================================================================
 
 Section 4: External Files
 
         [ Node 1 ]
         
         Connect.WAV
         [                                     ]
         
         Disconnect.WAV
         [                                     ]
         
         Error.WAV
         [                                     ]
         
         Connect display file *
         [                                     ]
         
         Disconnect display file *
         [                                     ]
         
         Error display file *
         [                                     ]
         
 * meaning not used or disabled.
 
 While this section does offer sound, I noticed it didn't work. Personally
 I would recommend to disable this if you like getting a good night's sleep.
 
 ===========================================================================
 
 Section 5: Backup
 
                              [ Backup ]         [ Restore ]

 Make a Back up of your configuration or Re-store your settings. Pretty
 handy...
 
 ===========================================================================
 
 Setting up your BBS Software.
 
 I need to speak in General as every BBS software package is different and
 some are easier than others.
 
 NodeModem (Demo/Shareware) version needs to be NODE 1
 
 What I did for my regular dial-in users. I configured my Front-end Mailer
 and BBS software as Node 2 and made Node 1 a "Telnet" only node.
  
ώ SPITFIRE ready for use at 4:18 a.m. on Thu., Sep. 23, 1999.
  >>>>>>><<<<<<<        SPITFIRE Bulletin Board System         >>>>>>><<<<<<<
  >>>>>>><<<<<<<            Buffalo Creek Software             >>>>>>><<<<<<<
  >[ PAGE ON  ]<    Copyright (C) by Mike Woltz, 1987-1996     [ PRINT OFF  ]
  >>>>>>><<<<<<<           Press HOME Key For Help             >>>>>>><<<<<<<
ώ 16550 UART detected.
ώ SPITFIRE home path is C:\SF
ώ Work files path is C:\SF\WORK
ώ Display files path is C:\SF\DISPLAY
ώ Message files path is C:\SF\MESSAGE
ώ External protocol files path is C:\SF\EXTNOD1
ώ Initializing system at 57600 bps.
OK

ώ SPITFIRE ready for use at 4:20 a.m. on Thu., Sep. 23, 1999.
 ΥΝ[ SPITFIRE NODE 1 ASYNC CONFIGURATION ]ΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΈ
 ³                                                                          ³
 ³ <I> Initialization String                                                ³
 ³     ATS0=)V1Q0E0H0M0S2=1X1^M                                             ³
<³ <A> Answer String.................. : ATA                                ³
<³ <F> FAX Connection Result Msg...... : +FCO      <1> Line COM1.. : IRQ4   ³
<³ <P> Pre-Initialization String...... : ATZ^M     <2> Line COM2.. : IRQ3   ³
<³ <O> Off Hook String................ : ATM0H1    <3> Line COM3.. : IRQ9   ³
<³ <S> Serial Port No................. : 3         <4> Line COM4.. : IRQ3   ³
<³ <B> System Baud Rate............... : 57600     <5> Line COM5.. : IRQ4   ³
 ³ <E> Error Correction Message....... : ARQ       <6> Line COM6.. : IRQ0   ³
I³ <H> DTE Locked..................... : Yes       <7> Line COM7.. : IRQ0   ³
Y³ <N> Number Of Rings................ : 1         <8> Line COM8.. : IRQ0   ³
M³ <D> Display Result Messages........ : On       <F1> Base COM1.. : 03F8   ³
 ³ <C> Disconnect Delay............... : 28       <F2> Base COM2.. : 02F8   ³
A³ <U> Use High Speed Async Routines.. : No       <F3> Base COM3.. : 03E8   ³
 ³ <R> Baud Rate Requirement.......... : 0        <F4> Base COM4.. : 02E8   ³
S³ <L> Break Length..(1000=1 Second).. : 0        <F5> Base COM5.. : 03F8   ³
Y³ <M> DTR Hangup..................... : Yes      <F6> Base COM6.. : 0000   ³
Y³                                                <F7> Base COM7.. : 0000   ³
T³                                                <F8> Base COM8.. : 0000   ³
ώ³                   Enter Command or <Q>uit -                              ³
O³                                                                          ³
ώΤΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΎ

 ΥΝ[ SPITFIRE Bulletin Board System ]ΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΈ
 ³                                                                           ³
 ³      SPITFIRE Bulletin Board System is distributed under the shareware    ³
 ³ concept.  SPITFIRE can be utilized on a trial basis for not more than     ³
 ³ thirty (30) days.  In the event this software is used beyond the trial    ³
 ³ period, then the registration fee is required. You are free to distribute ³
 ³ SPITFIRE provided it remains in its original, unmodified condition and no ³
 ³ fee is charged.                                                           ³
 ³                                                                           ³
 ³      It is simple for you to register your copy of SPITFIRE.  Simply mail ³
 ³ $85.00 in U.S. funds (add $10.00 shipping & handling if outside of North  ³
 ³ America) and a completed registration form to the address shown below.    ³
 ³ Your registration fee will provide you a license to operate SPITFIRE.     ³
 ³                                                                           ³
 ³                            Buffalo Creek Software                         ³
 ³                               913 - 39th Street                           ³
 ³                          West Des Moines, Iowa 50265                      ³
 ³                                                                           ³
 ³           Call Buffalo Creek's BBS at (515) 225-8496 for support.         ³
 ΤΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΝΎ
Thank you for using SPITFIRE.

C:\sf>
  
 Here is my batch file to run the node.
 
 REM : Note below is the IP-Redirection software I use for darktech.org 
 REM : After connecting with my provider or NetZero
 REM
 cd\mannadt
 mannadt
 REM
 REM
 cd\netmodem
 netmodem
 cd\adf
 adf com3 3e8 9 57600 8192 8192 8
 cd \sf
 SET WCPORTID=3
 SET WCNODEID=1
 SET WCIRQID=9
 SET WCBASEID=3e8
 spitfire
 cd\adf
 adf unload
 
 Here is the view from ZOC my telnet Client.
 
 ***
 *** CONNECT TO N/A
 *** date 23.09.1999
 *** time 04:15:36
 ***
 
 [TELNET] CONNECT (dialup-209.245.76.27.LosAngeles1.Level3.net/209.245.76.27)
 NetModem/32 - Server
 Version 2.0/Alpha.sL (Build-2)
 Copyright 1997-1999 Dedrick Allen
 
 Registered To: Unregistered!
 
 ώ Error correction modem detected.
 
 Your Sysop is Al Robres - Node 1
 SPITFIRE Bulletin Board System - Version 3.51
 Buffalo Creek Software
 Copyright (C) by Mike Woltz, 1987-1996
 
 Do you want ANSI COLOR GRAPHICS? [y/N] Yes
 
 Enter your first name: Al
 Enter your last name: Robres
 Searching for Al Robres, please stand by...
 Enter your password: *****
 
 Al, do you wish to review the message statistics? [Y/n]? Yes
 
 Reviewing queued message conferences, please stand by.
 
 Message conference #1>>>>> MESSAGE QUEUE STATISTICS <<<<<
 Total Messages Scanned.......... : 0
 Total New Messages Scanned...... : 0
 
 TO YOU:
    New Messages To You.......... : 0
    Received Messages To You..... : 0
 
 FROM YOU........................ : 0
 
 Al, you have no messages.
 < ENTER >           
 Good morning, Al, welcome back.
 You are caller number 0,004.
 You last called on 09-23-99 at 04:10.
 There have been 3 calls today.
 You have called 3 other times today.
 You have called 3 times.
 You are allowed 60 minutes per day.
 You have 28 minutes left today.
 You are allowed 28 minutes this call.
 1 callers access this BBS.
 Your security level is 10.
 < ENTER >           
 List new files since last check? [y/N] Yes
 
 Searching File Area - #1 "Untitled File Area"
 
 < ENTER >           There are no bulletins today.

 >>>>>>>>> MAIN MENU <<<<<<<<<
 <M>.......... Message Section         <F>............. File Section
 <D>............. Door Section         <B>................ Bulletins
 <C>......... Comment To Sysop         <#>...... List Active Callers
 <L>.......... Locate A Caller         <W>....... Who's On/Node Chat
 <T>........This System's Info         <N>...... SPITFIRE Newsletter
 <P>........... Page The Sysop         <G>........ Goodbye & Log Off
 <X>........ Xpert Mode Toggle         <Y>.......... Your Statistics
 <O>.... Other Bulletin Boards         <A>......... Add BBS Name & #
 <?>....... HELP With Commands         
 
 It is presently 4:16 a.m. on Thu., Sep. 23, 1999.
 You have been on 0 minutes with 28 remaining.
 MAIN MENU - [M F D B C # L W T N P G X Y O A ?]? W
  
 >>>>>>>>> MAIN MENU <<<<<<<<<
 <M>.......... Message Section         <F>............. File Section
 <D>............. Door Section         <B>................ Bulletins
 <C>......... Comment To Sysop         <#>...... List Active Callers
 <L>.......... Locate A Caller         <W>....... Who's On/Node Chat
 <T>........This System's Info         <N>...... SPITFIRE Newsletter
 <P>........... Page The Sysop         <G>........ Goodbye & Log Off
 <X>........ Xpert Mode Toggle         <Y>.......... Your Statistics
 <O>.... Other Bulletin Boards         <A>......... Add BBS Name & #
 <?>....... HELP With Commands         
 
 It is presently 4:16 a.m. on Thu., Sep. 23, 1999.
 You have been on 1 minute with 27 remaining.
 MAIN MENU - [M F D B C # L W T N P G X Y O A ?]? G
 
 Are you SURE you want to log off [Y/n]? Yes
 
 SPITFIRE Bulletin Board System - Version 3.51
 You were logged on 1 minute.
 You have 27 minutes remaining today.
 Thank you for calling, Al.
 [TELNET] INFO: DISCONNECTED
  
 SESSION STATISTICS:
 
    Online Time:  00:01.41
    Cost:         0.12
 
                    Read    Write
    Session         6565       39
    Up/Download        0        0
    TOTAL           6565       39
 
 ***
 *** DISCONNECT
 *** time 04:17:18
 ***
                  
~~~ ReneWave v2.00+
--- Renegade v05-11 Exp
 * Origin: Telnet://dognet.darktech.org       Covina,Ca USA (58:800/802)
